### Navigation

- index
- modules |
- PySptools 0.13.0 beta documentation »

# Denoising classes

## MNF

class `noise.``MNF`

  Transform a HSI cube.

  `apply`(M)

    A linear transformation that consists of a noise whitening step and one PCA rotation.

    This process is designed to
      - determine the inherent dimensionality of image data,
      - segregate noise in the data,
      - allow efficient elimination and/or reduction of noise, and
      - reduce the computational requirements for subsequent processing.
    Parameters:
      M: numpy array
        A HSI cube (m x n x p).
    Returns: numpy array
      A MNF transformed cube (m x n x p).
    References:
      C-I Change and Q Du, “Interference and Noise-Adjusted Principal Components Analysis,” IEEE TGRS, Vol 36, No 5, September 1999.
  `display_components`(n_first=None, suffix=None)

    Display some bands.

    Parameters:
      n_first: int [default None]
        Display the first n components.
  `get_components`(n)
    Return: numpy array
      The n-th band (m x n x 1).
  `inverse_transform`(X)

    Inverse the PCA rotation step. The cube stay whitened. Usefull if you want to denoise noisy bands before the rotation.

    X: numpy array
      A transformed (MNF) cube (m x n x p).
    Return: numpy array
      A inverted cube (m x n x p).
  `plot_components`(path, n_first=None, suffix=None)

    Plot some bands.

    Parameters:
      path: string
        The path where to put the plot.
      n_first: int [default None]
        Print the first n components.

## SavitzkyGolay

class `noise.``SavitzkyGolay`

  Apply a Savitzky Golay low pass filter.

  `denoise_bands`(M, window_size, order, derivative=None)

    Apply the Savitzky Golay filter on each band.

    Parameters:
      M: numpy array
        A HSI cube (m x n x p).
      window_size: int
        the length of the window. Must be an odd integer number.
      order: int
        the order of the polynomial used in the filtering. Must be less then window_size - 1.
      derivative: string [default None]
        direction of the derivative to compute, can be None, ‘col’, ‘row’, ‘both’.
    Returns: numpy array
      the smoothed signal (or it’s n-th derivative) (m x n x p).
    Code source:
      The scipy Cookbook, SavitzkyGolay section. This class is not under the copyright of this file.
  `denoise_spectra`(M, window_size, order, deriv=0, rate=1)

    Apply the Savitzky Golay filter on each spectrum. Smooth (and optionally differentiate) data with a Savitzky-Golay filter. The Savitzky-Golay filter removes high frequency noise from data. It has the advantage of preserving the original shape and features of the signal better than other types of filtering approaches, such as moving averages techniques.

    Parameters:
      M: numpy array
        A HSI cube (m x n x p).
      window_size: int
        the length of the window. Must be an odd integer number.
      order: int
        the order of the polynomial used in the filtering. Must be less then window_size - 1.
      deriv: int [default 0]
        the order of the derivative to compute (default = 0 means only smoothing).
    Returns: numpy array
      the smoothed signal (or it’s n-th derivative) (m x n x p).
    Code source:
      The scipy Cookbook, SavitzkyGolay section. This class is not under the copyright of this file.
  `display_bands_sample`(band_no, suffix=None)

    Display a filtered band.

    Parameters:
      band_no: int or string
        The band index. If band_no == ‘all’, plot all the bands.
      suffix: string [default None]
        Add a suffix to the title.
  `display_spectrum_sample`(M, x, y, suffix=None)

    Display a spectrum sample with the original and the filtered signal.

    Parameters:
      M: ‘numpy array’
        The original cube (m x n x p).
      x: int
        The x coordinate.
      y: int
        The y coordinate.
      suffix: string [default None]
        Add a suffix to the title.
  `plot_bands_sample`(path, band_no, suffix=None)

    Plot a filtered band.

    Parameters:
      path: string
        The path where to put the plot.
      band_no: int or string
        The band index. If band_no == ‘all’, plot all the bands.
      suffix: string [default None]
        Add a suffix to the file name.
  `plot_spectrum_sample`(M, path, x, y, suffix=None)

    Plot a spectrum sample with the original and the filtered signal.

    Parameters:
      M: ‘numpy array’
        The original cube (m x n x p).
      path: string
        The path where to put the plot.
      x: int
        The x coordinate.
      y: int
        The y coordinate.
      suffix: string [default None]
        Add a suffix to the file name.

## Whiten

class `noise.``Whiten`

  Whiten the cube.

  `apply`(M)

    Whitens a HSI cube. Use the noise covariance matrix to decorrelate and rescale the noise in the data (noise whitening). Results in transformed data in which the noise has unit variance and no band-to-band correlations.

    Parameters:
      M: numpy array
        A HSI cube (m x n x p).
    Returns: numpy array
      A whitened HSI cube (m x n x p).
  `get`()
    Returns: numpy array
      The whitened HSI cube (m x n x p).

### Navigation

- index
- modules |
- PySptools 0.13.0 beta documentation »